### Adjustments

#### PEDAL HEIGHT AND FREE-PLAY

On all vehicles and clutch type operating systems, refer to the "Clutch Specifications Chart'' for clutch pedal height above floor and pedal free-play.

On all models with a hydraulically operated clutch system––pedal height is usually adjusted with a stopper limiting the upward travel of the pedal. Pedal free-play is adjusted at the master cylinder pushrod. If the pushrod is non-adjustable, free-play is adjusted by placing shims between the master cylinder and the firewall.

On all models with a mechanical clutch system follow the service procedure below:

1. Loosen the locknut and adjust the pedal height by means of the pedal stopper. Tighten the locknut.
2. Push the withdrawal lever (refer to the illustration of "B'' area) in by hand until resistance is felt. Adjust withdrawal lever play at the lever tip end with the locknuts. Withdrawal lever play should be 0.08–0.12 inch (23mm).
3. Depress and release the clutch pedal several times and then recheck the withdrawal lever play again. Readjust if necessary.
4. Measure the pedal free travel at the center of the pedal pad.

   Fig. 1: Clutch adjusting points — 200SX

   Fig. 2: Clutch pedal free height and free play — 1984 Stanza

   Fig. 3: Adjusting clutch pedal — 1987 Stanza

   Fig. 4: Adjusting clutch interlock switch — 1987 Stanza