### Maintenance Reminder Lights

#### RESETTING

On models with a sensor relay, reset the relay by pushing or inserting a small screwdriver into the reset hole. Reset relay at 30,000 and 60,000 miles. At 90,000 miles, locate and disconnect warning light wire connector.

On models without sensor light relay and Canada models locate and disconnect the warning light harness connector. The reminder light will no longer function. Refer to the illustrations.

Fig. 1: Oxygen sensor warning lamp harness connector 1982–83 200SX

Fig. 2: Oxygen sensor warning lamp harness connector 1984 200SX

Fig. 3: Sensor relay location 1985–87 200SX

Fig. 4: Oxygen sensor warning lamp harness connector 1985–87 200SX

Fig. 5: Resetting the oxygen sensor warning light — 200SX

Fig. 6: Disconnecting and resetting the oxygen sensor warning lamp 1984–87 Stanza (except station wagon)