#### ADJUSTMENT

Adjust the clearance between the brake pedal and the stop lamp switch or the ASCD switch, by loosening the locknut and adjusting the switch. The clearance should be approximately 1.0mm for 1982–84 Stanza or 0.30–1.00mm for 1985–92 Stanza and all other models. Use this service procedure as a guide if necessary.

NOTE: The stop light switch is adjusted so that the switch is not activated when the brake pedal is relaxed.