#### THROTTLE CABLE — FUEL INJECTED ENGINE

NOTE: The throttle cable is operated via a cam on the throttle shaft of the injection unit. The adjustment is located on the side of the air intake plenum.

1. Loosen the 2 lock-nuts that position the cable. Open the throttle lever and hold it at the fully open position.
2. Back off both lock-nuts. Slide the outer cable as far as it will go away from the throttle cam.
3. Turn the nut on the side away from the throttle until it just starts to hold. Then, back it off 3⁄4 1 1⁄4 revolutions. Tighten the nut on the throttle side to lock this position securely.