#### WHEEL SENSOR CLEARANCE ADJUSTMENT

Fig. 1: Checking rear wheel sensor-to-rotor clearance — 240SX model

1. Install the rear wheel sensor.
2. Check the clearance between the edge of the sensor and rotor teeth using a feeler gauge. Clearances should be as follows:
   1. On 240SX, rear wheel sensor clearance should 0.0138–0.0246 in. (0.035–0.625mm).
   2. On Stanza, the clearance should be 0.008–0.039 in. (0.2–1.0mm).
3. To adjust the clearance, loosen the sensor mounting bolt(s) and move the sensor back and forth until the clearance is as specified.
4. Once the clearance is set, tighten the sensor mounting bolt(s) to 13–20 ft. lbs.

   BRAKE SPECIFICATIONS