#### DRIVESHAFT VIBRATION

To check and correct an unbalanced driveshaft, proceed as follows:

1. Remove the undercoating and other foreign material which could upset shaft balance. Roadtest the vehicle.
2. If vibration is noted, disconnect driveshaft at differential carrier companion flange, rotate companion flange 180°degrees and reconnect the driveshaft.
3. Roadtest the vehicle, if vibration still exists replace driveshaft assembly. Note that driveshaft should be free of dents or cracks and run-out should not exceed 0.6mm.