### Transverse Link

#### REMOVAL & INSTALLATION

##### Stanza Wagon 4WD

Fig. 1: Transverse link removal — Stanza Wagon 4WD

1. Raise and support the rear of the vehicle on jackstands.
2. Before removing transverse link retaining bolts, matchmark the toe-in adjustment. Refer to the illustrations.
3. Remove the link retaining bolts.
4. Installation is the reverse of the removal procedure. Final tightening of the transverse link mounting bolts should take place with the wheels on the ground and the vehicle unladen. Check rear alignment.