### Power Steering Pump

#### REMOVAL & INSTALLATION

1. Remove the hoses at the pump and plug the openings shut to prevent contamination. Position the disconnected lines in a raised attitude to prevent leakage.
2. Remove the pump belt.
3. Loosen the retaining bolts and any braces, and remove the pump.
4. Installation is the reverse of removal procedure. Use the following torque specifications as a guide pulley lock-nut 23–31 ft. lbs. and pump bracket to engine 20–26 ft. lbs. Adjust the belt — refer to Section 1. Bleed the system.