### Actuator

#### REMOVAL & INSTALLATION

1. Relieve the pressure from the ABS system.
2. Disconnect the negative battery cable.
3. Disconnect the electrical harness connectors from the actuator.
4. Disconnect the fluid lines from the actuator. Plug the ends of the lines to prevent leakage.
5. On 240SX, remove the relay bracket.
6. Remove the actuator mounting bolts and nuts.
7. Remove the actuator from the mounting bracket.

   To install:

8. Position the actuator onto the mounting bracket.
9. Install the actuator mounting fasteners.
10. On 240SX, install the relay bracket.
11. Connect the fluid lines and the harness connectors.
12. Connect the negative battery cable.
13. Bleed the brake system.