### Fuel Filter

#### REMOVAL AND INSTALLATION

##### All Models

CAUTION
Make sure to relieve the fuel system pressure on fuel injected engines before replacing the fuel filter.

1. Properly relieve fuel system pressure.
2. Disconnect the negative battery cable.
3. Loosen the fuel hose clamps and disconnect the hoses from the fuel filter.
4. Remove the bolt securing the filter to the bracket or just remove the filter from the bracket clips.
5. Remove the filter.

   To install:

6. Install the new filter and secure the filter in the bracket.
7. If necessary, replace the fuel line hoses and hose clamps. Reconnect the fuel hoses and tighten the clamps.
8. Reconnect the negative battery cable.
9. Install the fuel pump fuse.
10. Start the engine and check for leaks.