#### ALIGNMENT

The hood can be adjusted with bolts attaching the hood to the hood hinges, hood lock mechanism and hood bumpers. Adjust the hood for an even fit between the front fenders.

1. Adjust the hood fore and aft by loosening the bolts attaching the hood to the hinge and repositioning hood.
2. Loosen the hood bumper lock nuts and lower bumpers until they do not contact the front of the hood when the hood is closed.
3. Set the striker at the center of the hood lock, and tighten the hood lock securing bolts temporarily.
4. Raise the two hood bumpers until the hood is flush with the fenders.
5. Tighten the hood lock securing bolts after the proper adjustment has been obtained.

   Fig. 1: Adjusting hood at hinges

   Fig. 2: Adjusting hood at bumper rubber

   Fig. 3: Adjusting hood at lock