### Adjustments

#### THROTTLE WIRE — CA20 ENGINE

The throttle wire is adjusted by means of double nuts on the carburetor side.

1. Loosen the adjusting nuts at the carburetor throttle wire bracket.

   Fig. 1: Throttle wire adjustment

2. With the throttle fully opened, turn the threaded shaft inward as far as it will go and tighten the 1st nut against the bracket.
3. Back off the 1st nut 1⁄2 turns and tighten the 2nd nut against the bracket.
4. The throttle wire stroke between the threaded shaft and the cam should be 27.5–31.5mm.