### Clutch Cable

#### ADJUSTMENT

##### Sentra and 200SX

NOTE: When the clutch cable is replaced, depress the clutch pedal 50 times as a break in procedure before adjusting the free-play.

1. Loosen the adjusting knob at the transaxle as much that is needed to obtain a proper adjustment.
2. Adjust the pedal freeplay by turning the adjusting knob at the transaxle.
3. Measure the distance from the pedal resting position to the end of the free travel.
4. The free-play travel should be 0.42–0.59 inches (10.5–15mm).
5. Road test vehicle for proper operation.