### Power Steering Pump

#### BLEEDING

##### All Models

1. Raise and support the front of the vehicle safely.
2. Check and add fluid to the reservoir, if necessary.
3. Turn the steering wheel quickly (all the way), right and left, just touching the stops. Continue turning the steering wheel until the fluid level in the reservoir no longer decreases.
4. Check the fluid level, add fluid as required.
5. Start the engine and continue turning the steering wheel from right to left, lightly touching the stops until the fluid level in the reservoir no longer decreases.
6. Stop the engine and check the fluid level, add fluid as required.

   NOTE: When bleeding the system, make sure the temperature of the fluid reaches 140–176°F (60–80°C).

7. Repeat the steps until all of the air is bled from the system.
8. If the air cannot be bled from the system, turn and hold the steering wheel at each stop for at least 5 seconds but never more than 15 seconds.