### Brake Caliper

#### REMOVAL & INSTALLATION

##### Types CL11H, CL11HB, CL14B and CL9H Series Disc Brake Assembly

1. See the appropriate procedure and remove the brake pads.
2. Disconnect the parking brake cable and brake hose. Unscrew the mounting bolts and remove the caliper assembly.

   Fig. 1: Turn the piston counterclockwise to remove it from the caliper body

   Fig. 2: Prying off the ring from the inside of the piston — some rings may be the snapring type

   Fig. 3: Various CL11H caliper parts

   Fig. 4: After removing the ring, remove the spring cover, spring and seat

   Fig. 5: Remove the ring ``B'' with snapring pliers, then remove the key plate, push rod and rod

   Fig. 6: Remove the O-ring from the push rod — replace the O-ring during installation

   Fig. 7: Carefully remove the oil seal — replace it during assembly

   Fig. 8: Removing the return spring

3. Remove the pin bolts and separate the caliper body from the mounting support.
4. Using needlenosed pliers, turn the piston counterclockwise and remove it.
5. Pry out the ring from inside the piston. You can now remove the adjusting nut, the ball bearing, the wave washer and the spacers.
6. Installation is in the reverse order of removal. Replace all seals and O-rings. Tighten the caliper mounting bolts to 28–38 ft. lbs.