### Shock Absorber

#### REMOVAL & INSTALLATION

##### 200SX

1. Open the trunk and remove the cover panel if necessary to expose the shock mounts. Pry off the mount covers, if so equipped.
2. Remove the nut holding the top of the shock absorber. Unbolt the bottom of the shock absorber.
3. Remove the shock absorber.
4. Installation is the reverse of removal. Make sure rear shock retaining bushings and washer are installed in the correct position. Refer to the illustrations for additional specifications.

##### Stanza 2WD Wagon

1. Raise and support the rear of the vehicle on jackstands.
2. Remove the upper nut and the lower mounting bolt form the shock absorber.
3. Remove the shock absorber from the vehicle.
4. To install, reverse the removal procedures. Make sure rear shock retaining bushings and washer are installed in the correct position. Refer to the illustrations for additional specifications.

   Fig. 1: Rear suspension — Stanza 2WD