### Park/Neutral Safety Switch

#### REMOVAL AND INSTALLATION

1. Raise and support the vehicle safely.
2. Disconnect the manual control linkage from the manual shaft.
3. Disconnect the harness connectors from the park/neutral safety switch.
4. Remove the bolts that secure the switch to the side of the transfer case and remove the switch.

   To install:

5. Install the switch and secure with mounting bolts.
6. Connect the harness connectors to the park/neutral switch.
7. Set the manual shaft on the side of the transaxle to the N position.
8. Loosen the park/neutral switch mounting screws enough to allow for movement of the switch.
9. Insert a 0.16 in. (4 mm) diameter pin and move the switch until the pin falls through the locating hole in the inhibitor switch and manual shaft. Tighten the switch screws equally.

   Fig. 1: Control cable and adjustment pin

10. Remove the pin and connect the manual control linkage to the shaft.
11. Check for continuity at the park/neutral switch in the N, P and R ranges.
12. Make sure while holding the brakes on, that the engine will start only in P or N and that the backup lights only illuminate in reverse.