### Door Locks

#### REMOVAL & INSTALLATION

NOTE: Refer to the exploded view of Front and Rear Door Assembly.

1. Remove the door panel and sealing screen.
2. Remove the lock cylinder from the rod by turning the resin clip.
3. Loosen the nuts attaching the outside door handle and remove the outside door handle.
4. Remove the screws retaining the inside door handle and door lock, and remove the door lock assembly from the hole in the inside of the door.
5. Remove the lock cylinder by removing the retaining clip.

   To install:

6. Install the lock cylinder and clip to the door.
7. Install the door lock assembly and handles.
8. Install door panel and all attaching parts.

   Fig. 1: Lock cylinder assembly