### Windshield Washer Motor

#### REMOVAL & INSTALLATION

##### Front and Rear

Remove the washer reservoir/motor assembly from the vehicle and drain into a suitable container. Remove all connections. Pull the motor from the rubber grommet. If having difficulty, lubricate the grommet with penetrating oil and try again. Apply petroleum jelly to install the motor. Reconnect all connections.

Fig. 1: Washer hose routing

Fig. 2: Clean pivot area before installing wiper arm/blade

Fig. 3: Washer nozzle adjustment

Fig. 4: Washer system check valve