### Bumpers

#### REMOVAL & INSTALLATION

##### Front and Rear

Fig. 1: Bumper assembly — early models

1. Disconnect all electrical connectors at bumper assembly if so equipped.
2. Remove bumper mounting bolts and bumper assembly.
3. Remove shock absorbers from bumper.

   CAUTION
   The shock absorber is filled with a high pressure gas and should not be disassembled, drilled or exposed to an open flame.

4. Install shock absorbers and bumper in reverse order of removal.