#### BLEEDING PROCEDURE

The brake bleeding sequence varies from vehicle to vehicle and whether the vehicle is equipped with ABS or not. Bleeding sequences are as follows:

- 240SX (with ABS) — left rear caliper, right rear caliper, right front caliper, left front caliper, front side air bleeder on ABS actuator, rear side air bleeder on ABS actuator
- Stanza — left wheel cylinder or caliper, right front caliper, right rear wheel cylinder or caliper, left front caliper

To bleed the brakes, use the following procedure:

1. If equipped with ABS, turn the ignition switch to the OFF position and disconnect the connectors from the ABS actuator. Wait a few minutes to allow for the system to bleed down, then disconnect the negative battery cable.
2. Connect a transparent vinyl tube to the bleeder valve. Submerge the tube in a container half filled with clean brake fluid.
3. Fully depress the brake pedal several times.
4. With the brake pedal depressed, open the air bleeder valve to release the air.
5. Close the air bleeder valve.
6. Release the brake pedal slowly.
7. Repeat Steps 36 until clear fluid flows from the air bleeder valve.
8. Check the fluid level in the master cylinder reservoir and add as necessary.