### Injector Rubber Hose

#### REMOVAL & INSTALLATION

1. On injector rubber hose, measure off a point approximately 0.79 in. (20mm) from socket end.
2. Heat soldering iron (150 watt) for 15 minutes. Cut hose into braided reinforcement from mark to socket end.

   NOTE: Do not feed soldering iron until it touches injector tail piece. Be careful not to damage socket, plastic connector, etc. with solder iron. Never place injector in a vise when disconnecting rubber hose.

3. Pull rubber hose out with hand.

   To install:

4. Clean exterior of injector tail piece.
5. Wet inside of new rubber hose with fuel.

   Fig. 1: Removing the fuel injector hose

6. Push end of rubber hose with hose socket onto injector tail piece by hand as far as it will go. Clamp is not necessary at this connection.

   NOTE: After properly connecting fuel hose to injector, check connection for fuel leakage.