### Door Panel, Glass and Regulator

#### REMOVAL & INSTALLATION

##### Front and Rear

NOTE: Refer to the exploded view of Front and Rear Door Assembly.

1. Remove the regulator handle by pushing the set pin spring off.
2. Remove the arm rest, door inside handle escutcheon and door lock.
3. Remove the door finisher and sealing screen.
4. On some models it may be necessary to remove the outer door molding.
5. Lower the door glass with the regulator handle until the regulator-to-glass attaching bolts appear at the access holes in the door inside panel.
6. Raise the door glass and draw it upwards.
7. Remove the regulator attaching bolts and remove the regulator assembly through the large access hole in the door panel.

   To install:

8. Install the window regulator assembly in the door.
9. Connect all mounting bolts and check for proper operation.
10. Adjust the window if necessary and install the door trim panel.
11. Install all the attaching components to the door panel.
12. Install the window regulator handle.

    Fig. 1: Removing outer door molding

    Fig. 2: Removing glass attaching bolts

    Fig. 3: Removing window regulator from the door

    Fig. 4: Regulator handle and set pin removal and installation

    Fig. 5: Front door assembly — 1988 200SX

    Fig. 6: Front door assembly — early models

    Fig. 7: Rear door assembly — early models

    Fig. 8: Rear door assembly — late models

    Fig. 9: Front door assembly — late models

    Fig. 10: Rear door assembly —1992 Stanza

    Fig. 11: Front door assembly — 1992 Stanza