### Actuator

#### REMOVAL & INSTALLATION

1. Disconnect the negative battery cable.
2. Disconnect the Automatic Speed Control Device (ASCD) cable from the actuator assembly.
3. Disconnect vacuum hose from ASCD release valve.
4. Remove bolts attaching the actuator assembly to the body of the vehicle.
5. Installation is the reverse of the removal procedures. Adjust the ASCD cable as required. Check system for proper operation.