#### ADJUSTMENT PROCEDURE

##### 1982–83 Stanza 49 States Models 1984–85 Stanza Canadian Models

NOTE: Always refer to the underhood specifications sticker for any additional applicable procedures.

1. Connect a tachometer to the engine according the manufacturer's instructions.
2. Start the engine and run it until it reaches normal operating temperatures.
3. Operate it at 2,000 rpm for 2 minutes under no load, then idle for 1 minute.

   NOTE: If the cooling fan is operating, wait until it stops.

4. If equipped with a manual transaxle, place the shift selector in NEUTRAL; if equipped with an automatic transaxle, place the shift selector in DRIVE.
5. If the idle speed is not correct, adjust the throttle adjusting screw at the carburetor.
6. When the idle speed is correct, stop the engine and disconnect the tachometer.

   Fig. 1: Adjusting idle speed — Stanza