### Heater Water Control Valve

#### REMOVAL & INSTALLATION

##### All Models

1. Disconnect the negative battery cable.
2. Drain the cooling system. Remove all the necessary components in order to gain access to the valve retaining assembly.
3. Disconnect the electrical, vacuum or mechanical connections from the valve.
4. Disconnect the heater hose from the valve. Remove the control valve from the vehicle.
5. Installation is the reverse of the removal procedure. Refill the cooling system––bleed system if necessary. Check system for proper operation.