### Rear Wiper Motor

#### REMOVAL & INSTALLATION

Fig. 1: Rear window wiper motor — 1983 200SX

1. Disconnect the negative battery cable. Position the wiper arm to raise the wiper blade off the rear window glass. Then, remove the attaching nut and washers; then, work the wiper arm off the motor shaft.
2. Remove the attaching screws and remove the hatchback/liftback area inner finish panel. Carefully peel the plastic water shield off the sealer if so equipped.
3. Disconnect the electrical connector at the motor. Remove the motor mounting bolts and remove the motor.
4. Install the motor in reverse of the removal procedure. Torque the rear window wiper arm-to-motor nut to 9–13 ft. lbs. (13–18 Nm).
5. Before installing the water shield, run a fresh ring of sealer around the outer edge if necessary.