#### REMOVAL AND INSTALLATION

##### Sentra and 200SX

1. Disconnect the negative battery cable.
2. Remove the air cleaner duct and air cleaner.
3. Loosen the idler pulley locknut and turn the adjusting nut counterclockwise, in order to remove the power steering belt.
4. Remove the drive belt from the air conditioning compressor.
5. Loosen the power steering hoses at the pump and remove the bolts holding the power steering pump to the bracket.
6. Disconnect and plug the power steering hoses and remove the pump from the vehicle.

   To install:

7. Install the power steering pump and connect hoses. Hand-tighten the power steering hoses at this time.
8. Tighten the power steering pump mounting bolts to specifications.
9. Install the A/C and power steering drive belts. Adjust the drive belt tension.
10. Finish tightening the power steering hoses.
11. Connect the negative battery cable and fill the power steering reservoir with Dexron II® automatic transmission fluid.
12. Bleed the power steering system by turning the steering wheel from side-to-side with the engine running. Verify that there are no power steering system fluid leaks.

##### Maxima, Altima, 300ZX and 240SX

1. Disconnect the negative battery cable.
2. If necessary, remove the air cleaner duct and the air cleaner.
3. Remove the drive belt from the air conditioning compressor, if equipped.
4. Loosen power steering pump belt adjustment as follows:
   1. Loosen the pivot and mounting bolts.
   2. Loosen the idler pulley locknut and turn the adjusting nut counterclockwise to remove the power steering belt.
5. Loosen the power steering hoses at the pump and remove the bolts holding the power steering pump to the bracket.
6. Disconnect and plug the power steering hoses and remove the pump from the vehicle.

   To install:

7. Using new O-rings, connect the power steering hoses to the steering pump.
8. Install the power steering pump and secure it with its mounting bolts. Tighten the front and rear mounting bolts to specifications.
9. Install the remaining components in the reverse order from which they were removed.
10. Connect the negative battery cable.
11. Fill the power steering system, start the engine and turn the steering wheel from side-to-side to bleed air from system.