## INSTRUMENTS AND SWITCHES

### Instrument Cluster/Combination Meter

#### REMOVAL & INSTALLATION

##### 200SX and 240SX

Fig. 1: Instrument panel — 1982 200SX

Fig. 2: Electronic digital instrument cluster assembly — 1984 200SX

Fig. 3: Instrument panel — Stanza

1. Disconnect the negative battery cable. Refer to illustrations.
2. Remove the steering wheel and steering wheel covers, as required.
3. Remove the screws holding the cluster lid in place and remove the lid.
4. On the 200SX, remove the 2 screws and 7 pawls to release the cluster. On the 240SX, the cluster is held with 3 screws.
5. Carefully withdraw the cluster assembly from the instrument panel and disconnect the speedometer cable (analog) and electrical wiring from the rear of the cluster. Make sure the wiring is labeled clearly to avoid confusion during installation.
6. Remove the cluster. Be careful not to damage the printed circuit.
7. Installation is the reverse of the removal procedure.

##### Stanza

1. Disconnect the negative battery cable. Refer to illustrations.
2. Remove the steering wheel and the steering column covers.
3. Remove the instrument cluster lid by removing its screws.
4. Remove the instrument cluster screws.
5. Gently withdraw the cluster from the instrument pad and disconnect all wiring and speedometer cable. Make sure the wires are marked clearly to avoid confusion during installation. Be careful not to damage the printed circuit.
6. Remove the cluster.
7. Installation is the reverse of removal.