### Crankshaft Damper

#### REMOVAL & INSTALLATION

To remove the crankshaft damper matchmark the crankshaft pulley to the damper. Remove the crankshaft pulley (outside) retaining bolts if so equipped. Remove the (center) crankshaft pulley to damper bolt, the use a puller tool to remove the pulley/damper from the crankshaft. When installing the damper and crankshaft pulley torque the center bolt to the correct specification.

Fig. 1: Removing crankshaft pulley with puller