## FIRING ORDERS

Fig. 1:Z-series engines Firing order: 1–3–4–2 Distributor rotation: counterclockwise

Fig. 2: CA20E engine Firing order: 1–3–4–2 Distributor rotation: counterclockwise

Fig. 3: VG30E engine Firing order: 1–2–3–4–5–6 Distributor rotation: counterclockwise

Fig. 4: KA24E engine (Stanza FWD) Firing order: 1–3–4–2 Distributor rotation: counterclockwise

Fig. 5: KA24E and KA24DE engines (240SX RWD) Firing order: 1–3–4–2 Distributor rotation: counterclockwise

NOTE: To avoid confusion, remove and tag the wires one at a time, for replacement.