#### ALIGNMENT

1. Loosen the trunk lid hinge attaching bolts until they are just loose enough to move the trunk lid.
2. Move the trunk lid for and aft to obtain a flush fit between the trunk lid and the rear fender.
3. To obtain a snug fit between the trunk lid and weather-strip, loosen the trunk lid lock striker attaching bolts enough to move the lid, working the striker up and down and from side to side as required.
4. After the adjustment is made tighten the striker bolts securely.

   Fig. 1: Trunklid assembly