#### ALIGNMENT

1. Open the hatchback lid.
2. Loosen the lid hinge to body attaching bolts until they are just loose enough to move the lid.
3. Move the lid up and down to obtain a flush fit between the lid and the roof.
4. After adjustment is completed tighten the hinge attaching bolts securely.

   Fig. 1: Hatchback assembly — 1988 200SX shown

   Fig. 2: Common tailgate assembly

   Fig. 3: Typical hatchback assembly