### Engine Fan

#### REMOVAL & INSTALLATION

##### Belt Drive Type (Engine)

Fig. 1: Engine fan assembly

Fig. 2: Checking clutch fan or coupling operation

1. Disconnect the negative battery cable.
2. Remove the fan shroud.
3. Remove the drive belt, fan assembly/pulley retaining bolts.
4. Remove the fan assembly.
5. Installation is the reverse of the removal procedure. Check fan coupling for rough operation before installation. Adjust the drive belt.

   NOTE: If necessary remove the radiator from the vehicle––refer to the necessary service procedure for additional clearance to remove the fan assembly.

##### Electric Type (Radiator Fan)

1. Disconnect the negative battery cable.
2. Unplug the condenser and radiator fan motor wiring harness connectors.
3. Remove the radiator shroud bolts.
4. Separate the shroud and cooling fan assembly from the radiator and remove.

   To install:

5. Mount the radiator shroud and cooling fan assembly onto the radiator.
6. Install the radiator shroud bolts.
7. Plug in the radiator and condenser fan motor harness connectors.
8. Connect the negative battery cable.