### Clutch Master Cylinder

#### REMOVAL & INSTALLATION

1. Disconnect the clutch pedal arm from the pushrod.
2. Disconnect the clutch hydraulic line from the master cylinder.

   NOTE: Take precautions to keep brake fluid from coming in contact with any painted surfaces.

3. Remove the nuts attaching the master cylinder and remove the master cylinder and pushrod toward the engine compartment side.
4. Install the master cylinder in the reverse order of removal and bleed the clutch hydraulic system.

   Fig. 1: Hydraulic clutch control — all models