### Antenna

#### REMOVAL & INSTALLATION

##### Fender Mounted (Fixed)

1. Remove antenna mounting nut.
2. Disconnect the antenna lead at the radio.
3. Remove antenna from vehicle.
4. Installation is in the reverse order of removal.

##### Power Antenna

1. Remove the antenna nut and antenna base.
2. Remove the antenna rod while raising it by operating antenna motor. Turn radio switch from OFF to ON to operate antenna motor.

   To install:

3. Lower antenna rod by operating antenna motor.
4. Insert gear section of antenna into place with it facing (see illustration) in the correct position for proper operation.
5. Retract antenna rod completely-attach antenna rod into housing.
6. Install antenna nut and base, check for proper operation.

   Fig. 1: Antenna location — 240SX model

   Fig. 2: Antenna rod replacement — Step 1

   Fig. 3: Antenna rod replacement — Step 2

   Fig. 4: Antenna rod replacement — Step 3