#### REMOVAL & INSTALLATION

Never smoke when working around gasoline! Avoid all sources of sparks or ignition. Gasoline vapors are EXTREMELY volatile!

1. Disconnect the fuel lines from the fuel pump. Be sure to keep the line leading from the fuel tank up high to prevent the excess loss of fuel.
2. Remove the two fuel pump mounting nuts and the fuel pump assembly from the right side of the engine.
3. To install, use a new gasket, sealant and reverse the removal procedures. Torque the fuel pump bolts to 79 ft. lbs. Replace the fuel line hose clamps as necessary.

Fig. 1: Engine fuel pump — CA20 engine series

Fig. 2: Testing mechanical fuel pump