# BODY AND TRIM

## EXTERIOR

### Doors

#### REMOVAL & INSTALLATION

##### Front and Rear

1. Place a jack or stand beneath the door to support its weight.

   NOTE: Place a rag between the lower edge of the door and jack or stand to prevent damage to painted surface.

2. Remove door without hinge.
3. Remove the door hinge.
4. Installation is in the reverse order of removal.

   NOTE: When installing hinge, coat the hinge link with recommended multipurpose grease.

   Fig. 1: Removing mounting bolts from the door