### Diagnosis and Testing

#### IC IGNITION TYPE SYSTEM

All diagnosis and testing should be perform in order according to the service charts below. Perform all test in the order stated by the diagnosis charts. Battery voltage must be 11.5–12.5 volts before starting all test procedures.

Fig. 1: Ignition system diagnosis chart

Fig. 2: Ignition system diagnosis chart

Fig. 3: Ignition system diagnosis chart