#### ADJUSTMENT

##### Front and Rear

Proper door alignment can be obtained by adjusting the door hinge and door lock striker. The door hinge and striker can be moved up and down fore and aft in enlarged holes by loosening the attaching bolts.

NOTE: The door should be adjusted for an even and parallel fit for the door opening and surrounding body panels.

Fig. 1: Adjusting door striker

Fig. 2: Using special type tool to adjust hinge