### Chassis Greasing

The manufacturer doesn't install lubrication fittings in lube points on the steering linkage or suspension. On some replacement part applications you can buy metric threaded fittings to grease these points or use a pointed, rubber tip end on your grease gun. Lubricate all joints equipped with a plug, every 15,000 miles or once a year with NLGI No. 2 (Lithium base) grease. Replace the plugs after lubrication.