#### REMOVAL & INSTALLATION

##### Front Cable

1. Remove the parking brake console box.
2. Remove the heat insulator, if equipped.
3. Remove the front passenger seat, if required.
4. Disconnect the warning lamp switch plate connector.
5. Unbolt the lever from the floor.
6. Working from under the vehicle, remove the locknut, adjusting nut and equalizer.
7. Pull the front cable out through the compartment and remove it from the vehicle.

   NOTE: On some vehicles it may be necessary to separate the front cable from the lever by breaking the pin.

8. Installation is the reverse of the removal procedure. Adjust the lever stroke.

##### Rear Cable

1. Back off on the adjusting nut or equalizer to loosen the cable tension.
2. Working from underneath the vehicle, disconnect the cable at the equalizer.
3. Remove the cable lock plate from the rear suspension member.
4. Disconnect the cable from the rear brakes.
5. Disconnect the cable from the suspension arm.
6. Remove the cable.
7. Installation is the reverse of the removal procedure. Adjust the lever stroke.

   Fig. 1: Parking brake assembly — Stanza

   Fig. 2: Parking brake adjustment

   Fig. 3: Two common types of parking brake cables — most vehicles are similar