#### ADJUSTMENT

##### 1982–83 200SX

Without depressing the accelerator pedal, adjust the adjusting nut until cable free play is within 0.08–0.012 in. (2–3mm) at throttle lever. Tighten the locknut.

##### 1984–88 200SX, 240SX and Stanza (Vacuum Type)

1990–92 Stanza

Without depressing the accelerator pedal, adjust the adjusting nuts until there is no free play or portion A of throttle lever comes in contact with assembly. Then return adjustment (back off) nuts 1⁄2 –1 turn back to gain free play. Securely tighten lock nut to hold adjusting nut in place.

##### Stanza (Positive Pressure Type)

On the this type system, the actuator cable is operated by compressed air produced in the compressor built into the actuator assembly.

Without depressing the accelerator pedal, adjust the adjusting nuts until there is no free play––tighten lock nut.