#### 1984–88 200SX WITH THE CA20E, CA18ET AND VG30E ENGINES

NOTE: Starting in mid year 1986–88 the CA20E engine in the 200SX model valves are non-adjustable. On V6 equipped 200SX models the valves are also non-adjustable. Refer to Valve Clearance column in the Tune-Up Specifications Chart.

Valve adjustment should be made while engine is warm but no running. Follow the procedure above for 1982–83 models, with the following exceptions: on Step 4, check and adjust the clearance valves 1, 2, 4 and 6 as shown in the accompanying illustration. This is with No. 1 cylinder at TDC on compression. On Step 6, check and adjust the clearance on valves 3, 5, 7 and 8 with the No. 4 cylinder at TDC on compression.

Fig. 1: Adjusting valve clearance

Fig. 2: Valve location, 1984 and later 200SX (CA20E and CA18ET engines) — See text for procedure