### Clutch Slave Cylinder

#### REMOVAL AND INSTALLATION

1. Raise and safely support the vehicle.
2. Disconnect the flexible fluid hose from the slave cylinder.
3. Remove the slave cylinder attaching bolts.
4. Remove slave cylinder and pushrod.

   To install:

5. Install the slave cylinder and pushrod.
6. Install attaching bolts and torque to 22–30 ft. lbs. (30–40 Nm).
7. Connect the flexible fluid hose and tighten the fitting to 12–14 ft. lbs. (17–20 Nm).
8. Bleed system and check for leaks.
9. After bleeding the clutch system, tighten the bleeder screw to 52–86 inch lbs. (6–10 Nm).