#### COOLING SYSTEM BLEEDING

Fig. 1: Air relief plug — Stanza KA24E engine

Fig. 2: Air relief plug — 240SX KA24DE engine

1. Remove the radiator cap.
2. Fill the radiator and reservoir tank with the proper type of coolant. If equipped with an air relief plug, remove the plug and add coolant until it spills out the air relief opening. Install the plug.
3. Install and tighten the radiator cap.
4. Start the engine and allow the coolant to come up to operating temperature. If equipped allow the electric cooling fan to come on at least once. Run the heater at full force and with the temperature lever in the HOT position. Be sure the heater control valve is functioning.
5. Shut the engine off and recheck the coolant level, refill as necessary.