### Catalytic Converter

#### REMOVAL & INSTALLATION

1. Remove the converter lower shield.
2. Disconnect converter from front pipe.
3. Disconnect converter from center pipe.

   NOTE: Assemble all parts loosely and position converter before tightening the exhaust clamps.

4. Remove catalytic converter.
5. To install reverse the removal procedures. Always use new clamps and exhaust seals, start engine and check for leaks.