#### REMOVAL & INSTALLATION

1. Disconnect the negative battery cable from the battery.
2. Disconnect the starter wiring at the starter, taking note of the positions for correct installation.
3. Remove the bolts attaching the starter to the engine and remove the starter from the vehicle.

   To install:

4. Install the starter to the engine.
5. Tighten the attaching bolts EVENLY. Be careful not overtorque the mounting bolts as this will crack the nose of the starter case assembly.
6. Install the starter wiring in the correct location.
7. Connect the negative battery cable.
8. Start the engine a few times to make sure of proper operation.