### Wheel Bearings

#### REMOVAL, PACKING AND INSTALLATION

##### Rear Wheel Drive Vehicles

###### 200SX and 240SX MODELS

Clean, inspect and repack wheel front wheel bearings every 30,000 miles or 24 months on 1982–88 200SX rear wheel drive models. The 1989–92 240SX rear wheel drive models uses a one-piece style front wheel bearing assembly no maintenance is required.

In order to clean and repack the front wheel bearings on the 200SX rear wheel drive models the wheel bearings must be removed from the wheel hub. You should also check that the wheel bearings operate smoothly and their is no excess amount of play (looseness) in the bearing assembly before removing the wheel bearing. To remove, install and adjust the wheel bearings and for all other service procedures for "Front Wheel Bearings'' rear wheel drive vehicles refer to Section 8 in this manual.

##### Front Wheel Drive Vehicles

###### STANZA MODELS

On front wheel drive vehicles the front wheel bearings are different than on rear wheel drive vehicles and (front hub must be removed — bearing assembly pressed in and out) no normal maintenance is required. For service procedures (removal and installation) for "Front Wheel Bearings'' front wheel drive vehicles refer to Section 8 in this manual.

The rear wheel bearings on front wheel drive vehicles are similar to the front bearings on rear wheel drive vehicles. In order to clean and repack the rear wheel bearings on the Stanza front wheel drive models the wheel bearings must be removed from the wheel hub. Clean, inspect and repack wheel rear wheel bearings every 60,000 miles or 48 months. To remove, install and adjust the rear wheel bearings and for all other service procedures for "Rear Wheel Bearings'' front wheel drive vehicles refer to Section 8 in this manual.