#### ADJUSTMENT

1. Raise and support the vehicle on jackstands.
2. Loosen the inhibitor switch adjusting screws. Place the select lever in the Neutral position.

   Fig. 1: Adjusting the inhibitor switch

3. Using a 2.5mm diameter pin (RL3F01A type transaxle––early model Stanza) or a 4mm diameter pin (RL4F02A type transaxle––late model Stanza) place the pin into the adjustment holes on both the inhibitor switch and the switch lever (the switch lever should be as near vertical position as possible).
4. Tighten the adjusting screws EVENLY to 1.4–1.9 ft. lbs. Check the switch for continuity by making sure the vehicle starts only in P or N.